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PART 1 - GENERAL
1.1 SUMMARY
Provide, install, configure where applicable, test and commission the industrial ethernet media converter described in this specification, including the required interfaces, power connections, mounting hardware and compatible accessories.
1.2 BASIS OF DESIGN
Basis-of-design manufacturer and product: KBC Networks MCGN1-P1N. Source description: Industrial one channel 10/100/1000M Ethernet Media Converter With SFP.
Equivalent products may be considered only when they meet or exceed every stated interface, performance, power, environmental and mounting requirement without changing the intended system design.
1.3 SUBMITTALS
Manufacturer technical data sheet identifying the exact model and selected hardware variant.
Interface or connection schedule identifying the electrical, optical, wireless, power and network connections.
Power calculation confirming input-supply compatibility and the total connected load where applicable.
Mounting, environmental and configuration details applicable to the proposed installation.
1.4 QUALITY ASSURANCE
Installation shall be performed by personnel familiar with industrial Ethernet, copper and optical interfaces, PoE power budgeting, transceiver selection and applicable electrical and network practices. Verify all product capability from the current manufacturer data sheet and selected part number.
PART 2 - PRODUCTS
2.1 REQUIRED PRODUCT
The equipment shall be KBC Networks MCGN1-P1N, or an approved equivalent meeting all requirements below. It shall be supplied as industrial one channel 10/100/1000m ethernet media converter with sfp.
2.2 PRODUCT DESCRIPTION
The KBC MCGN1 series is an industrial 10/100/1000M Ethernet media converter. It supports transmission of one channel 10/100/1000 Base-T Ethernet over SFP port, by selecting different KBC SFP modules, the media converter can be transmitted via one or two, multimode or single mode optical fibers with full duplex operation. There is no A end or B end for MCLN1-P1N series, both ends of MCGN1-P1N are same , but when inserting 1 fiber version SFP module, two ends should be matched, that means one end is 1310nm/1550nm SFP, the other end is 1550nm/1310nm SFP. Plug-and-play design makes installation straightforward, with no electrical or optical adjustment needed. LED indicators are provided to show the operational status of the unit. Rugged design in both enclosure and electrical protection makes it suit for application in harsh environment.
The series is available in wall, DIN, and 2U passive rack FR2-12, or card version in 2U chassis FR2-16.
2.3 KEY FEATURES
10/100/1000M auto sensing port
1*10/100/1000Base-TX Port
1*1000Base-FX SFP Port
2kV Surge Protection on RJ45 electrical Port
Compatible with one channel MCGN1 series with 1*9 optics, two channel 10/100/1000M media converter MCGN2 series
IP40 enclosure
DIN, Wall Mount
FR2-12 passive Rack with 12 slots or Chassis card in FR2-16 with 16 slots
2.4 SOURCE-VERIFIED TECHNICAL REQUIREMENTS
	Requirement
	Specified performance

	Standards - IEEE Standards
	IEEE802.3, IEEE802.3u IEEE802.3ab,IEEE802.3z

	Environmental - Operating Temperature
	-40° ~ +75°C

	Environmental - Storage Temperature
	-40° ~ +85°C

	Environmental - Operating Humidity
	0 to 95% non-condensing

	Environmental - Mean Time Between Failure (MTBF)
	> 100,000 Hours

	Electrical - Data Port
	1

	Electrical - Data Rate
	10/100/1000Mbps Auto-Sensing Half & Full Duplex

	Environmental - Enclosure Protection
	IP40

	Electrical - Surge Protection
	2kV

	Connectors - 10/100/1000M Electrical
	RJ-45

	Connectors - Power (3) Wall Mount/DIN Rail
	Screw Block Terminal

	Optical - 1000Base-FX SFP Port (1)
	1

	Others - Cable
	CAT5 or CAT6, direct or cross cable

	Power - Power Input
	+12Vdc

	Others - LEDs
	Connection status data sending & receiving

	Power - Power consumption
	<3W

	Power - Power Supply (2)
	Input: 100 ~ 240Vac Output: +12Vdc

	Power - Chassis Card
	Supplied from FR2 PSU


The installer shall verify the selected part number, accessories and all project-specific operating limits against the current manufacturer data sheet before procurement and installation.
2.5 SOURCE VERIFICATION NOTE
The requirements in this document have been prepared from Specsheet-MCGN1-P1N_Series-Rev1803.pdf. Any configurable channel count, optical module, antenna, power supply, plug, mounting option, battery, solar array, accessory or regional variant shall be selected and confirmed separately where the source sheet presents multiple possibilities.
PART 3 - EXECUTION
3.1 EXAMINATION
Confirm that the proposed equipment and selected variant match the approved design, required interfaces and intended operating environment.
Confirm that all input-power, cable, fiber, antenna, network and mounting conditions are within the manufacturer limits.
Confirm that all required accessories, transceivers, power supplies, batteries, antennas, mounting components and interconnection items are available and compatible.
Do not begin installation until conflicts between the design, site conditions and manufacturer requirements have been resolved.
3.2 INSTALLATION
Confirm copper speed, duplex mode, optical speed, connector, wavelength, fiber type and link distance for each connection.
Provide approved fixed-optic or SFP transceivers matched to the intended optical path.
Provide compatible power, protective earthing, cable management and environmental protection.
Label each converter, power circuit, copper port and optical link to match the project documentation.
3.3 CONFIGURATION AND COMMISSIONING
Verify link operation on every connected copper and optical interface.
Verify PoE negotiation and delivered power at each powered device where applicable.
Confirm speed, duplex, link-fault and diagnostic behaviour supported by the selected model.
Provide final link schedules, test results and installed model/serial information.
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