

A & E SPECIFICATIONS	

KBC MOBILE SURVEILLANCE SYSTEM (MSS)
PART 1 - GENERAL
1.1 SUMMARY
Provide, install, configure (where applicable), test, and commission the industrial power solution described in this specification, including the required interfaces, power connections, mounting hardware, and compatible accessories.
1.2 BASIS OF DESIGN
Basis-of-design manufacturer and product: KBC Networks MSS. Source description: Mobile Surveillance System.
Equivalent products may be considered only when they meet or exceed every stated interface, performance, power, environmental and mounting requirement without changing the intended system design.
1.3 SUBMITTALS
Manufacturer technical data sheet identifying the exact model and selected hardware variant.
Interface or connection schedule identifying the electrical, optical, wireless, power and network connections.
Power calculation confirming input-supply compatibility and the total connected load where applicable.
Mounting, environmental and configuration details applicable to the proposed installation.
1.4 QUALITY ASSURANCE
Installation shall be performed by personnel familiar with industrial DC power systems, load calculations, battery or solar sizing, protective devices, environmental enclosures and applicable electrical practices. Verify all product capabilities from the current manufacturer data sheet and selected part number.
PART 2 - PRODUCTS
2.1 REQUIRED PRODUCT
The equipment shall be KBC Networks MSS, or an approved equivalent meeting all requirements below. It shall be supplied as a mobile surveillance system.
2.2 PRODUCT DESCRIPTION
Mobile Surveillance Systems (MSS) are self-contained solutions for monitoring locations that lack infrastructure, require time-sensitive deployment, are temporary or a combination of these factors. They are compact, rugged, and easy to operate. MSS units consist of a base unit with on-board solar panel(s), a charge controller and batteries (purchased separately), along with power and network connections for all connected devices. A removable quick-connect pod provides a mounting platform for cameras, wireless, radar or other systems.
MSS units are a force multiplier for management, security, medical, law enforcement or event personnel by providing the ability to monitor an area more efficiently and effectively. The systems are most effective when used in groups, as they can be easily linked together in perimeter, star, and linear configurations. Because of their size and maneuverability, MSS units provide a platform that can be deployed quickly in smaller areas and is less conspicuous than other solutions.
MSS-KT-300-15 operates in a variety of weather environments and includes multiple security features.
2.3 KEY FEATURES
Compact self-contained unit – maneuverable and easy to deploy
Industrial – vandal-resistant – low maintenance
Remote, mobile, cost-effective
Unique gas shock-assisted mast lift assembly – elevation up to 15 feet
Removable quick-connect interchangeable pods
Adjustable solar panel – gas shock-assisted lift deployable at multiple angles
MPPT Charge controller
Space for up to 3 x 110 Ah batteries in base (purchased separately)
Optional configurations and accessories are available
2.4 SOURCE-VERIFIED TECHNICAL REQUIREMENTS

	Requirement
	Specified performance

	Mechanical
	MSS-KT-300-15

	Stowed
	32” x 41” x 65”

	Deployed
	63” x 68” x 180”

	Shipping Weight
	400 lb (620 lb with batteries)

	Construction
	Steel Chassis

	Mast
	Swing-Arm Gas Spring Assist - Aluminum

	Steel/Aluminum Chassis
	Swing-Arm gas spring-assisted mast (1x 80 lb and 1x 60 lb) / 4x 10” pneumatic tires with steel hub with 300 lb capacity / 4x Adjustable outriggers and levelers / spring-assisted solar array (2x 60 lb)

	Wheels
	10” Pneumatic Tire/Steel Hub (4x) 300 lb Capacity Each

	Supports
	4 Adjustable Outriggers & Levelers

	Electronics Tray
	Fixed aluminum tray

	Solar Mount
	Adjustable with Pin Lock

	Mast Lift Mechanism
	1 – 80 lb & 1 - 60 lb Gas Spring

	Solar Lift Mechanism
	2 – 60 lb Gas Springs

	Quick-Connect Pod
	Aluminum w/ 12VDC & RJ45 Connector

	Finish
	Powder Coat - White

	Security Features - Base
	2x Key Lock/Removable Wheels

	Security Features - Mast
	Key Lock Latches

	Security Features - Quick-Connect Pod
	Key Lock Latch

	Power - Electrical
	12VDC System

	Power - Batteries
	3x – 110 Ah

	Power - Solar Panels
	3x - 100W Panels

	Power - Wiring
	Cat6e & 14 GWA 2-wire Internal to Mast & Base

	Power - Charge Controller
	MPPT 100/20 - Bluetooth Capable

	Quick-Connect Pod - Latches
	Standard & Key Lock

	Quick-Connect Pod - Wiring
	Cat6e/18 GWA 2-wire

	Quick-Connect Pod - Weatherproofing
	Square Rubber “O” Ring, Rubber Gasket


The installer shall verify the selected part number, accessories and all project-specific operating limits against the current manufacturer data sheet before procurement and installation.
2.5 SOURCE VERIFICATION NOTE
The requirements in this document have been prepared from MSS_Series-Specification_Sheet-2303.pdf. Any configurable channel count, optical module, antenna, power supply, plug, mounting option, battery, solar array, accessory or regional variant shall be selected and confirmed separately where the source sheet presents multiple possibilities.
PART 3 - EXECUTION
3.1 EXAMINATION
Confirm that the proposed equipment and selected variant match the approved design, required interfaces and intended operating environment.
Confirm that all input power, cable, fiber, antenna, network and mounting conditions are within the manufacturer limits.
Confirm that all required accessories, transceivers, power supplies, batteries, antennas, mounting components and interconnection items are available and compatible.
Do not begin installation until conflicts between the design, site conditions and manufacturer requirements have been resolved.
3.2 INSTALLATION
Confirm the continuous and peak load, input source, output voltage, required autonomy and environmental conditions.
Verify battery, solar-array, charger, controller, inverter or DC distribution compatibility where applicable.
Provide protective earthing, overcurrent protection, isolation, cable sizing and weatherproof entry arrangements.
Install all equipment, enclosures and mounting assemblies in accordance with manufacturer instructions and approved drawings.
3.3 CONFIGURATION AND COMMISSIONING
Verify input, charging, output voltage, and load performance under normal operating conditions.
Verify battery autonomy, solar charging or UPS transfer operation where applicable.
Demonstrate alarm, recovery and protection functions supported by the selected system.
Provide final power calculations, settings, test results and installed model/serial information.
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